|  |  |
| --- | --- |
| **WILD NATURE HD** | |
| **satellite** | Express-80 2 satellite, degree 80 |
| **Character speed** | 45 M/s |
| **polarization** | Vertical polarization |
| **frequency** | 11606 MHz |
| **FEC** | 4/5 |
| **Modulation** | QPSK (DVB-S2) |
| **number of audio tracks** | 2 (sounds of nature OR relaxing music) |
| **title language** | non-narrative with locations in English, Russian, French, Spanish, Arabic, Chinese on the screen |
| **Audio** | Stereo |
| **audio track codec** | MPEG-1 |
| **Broadcast format** | 16: 9 |
| **Resolution** | HD, 1080i |
| Output signal format - digital signal with no resolution less than 1920 × 1080 pixels in accordance with ISO / IEC 13818. | |
| The speed of the transmitted stream is not more than 15 Mbit / s per HQTV. | |
| The Licensor's channel signal is encoded for reception source # 1 and not encoded for other reception sources. | |